Eufy E40 Camera Housing – Installation Guide
Installing the camera into the internal holder

Step 1: Angle the front of the camera downward and place it into the camera holder.
Step 2: Slide the camera into the holder, straighten the camera, and then slide it forward until it is seated securely in the camera holder.
Note: The camera should sit level and snug inside the holder before the housing is closed.
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Did you know we have a website?
More designs and custom builds available on our

website.
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